# Virtual LANs

The term VLAN (Virtual Local Area Network) refers to a collection of devices that communicate as if they were on the same physical LAN. Any set of ports (including all ports on the switch) can be considered a VLAN. LAN segments are not restricted by the hardware that physically connects them.

| VLANs offer the ability to group computers together into logical workgroups. This can simplify network administration when connecting clients to servers that are geographically dispersed across the building, campus, or enterprise network. Typically, VLANs consist of co-workers within the same department but in different locations, groups of users running the same network protocol, or a cross-functional team working on a joint project.

By using VLANs on your network, you can:

- Improve network performance

- Limit broadcast storms

- Improve LAN configuration updates (adds, moves, and changes)

- Minimize security problems

- Ease your management task

## Other Considerations

- To set up IEEE VLAN membership (multiple VLANs), the adapter must be attached to a switch with IEEE 802.1Q VLAN capability.

- A maximum of 64 VLANs per network port or team are supported by Intel software.

- VLANs can co-exist with teaming. If you do this, the team must be defined first, then you can set up your VLAN.

- You can set up only one untagged VLAN per network port or team. You must have at least one tagged VLAN before you can set up an untagged VLAN.

| CAUTION: When using IEEE 802 VLANs, settings must match between the switch and those adapters using the VLANs.

### Microsoft* Load Balancing and Failover (LBFO) teams

Intel ANS VLANs are not compatible with Microsoft's LBFO teams. Intel® PROSet will block a member of an LBFO team from being added to an Intel ANS VLAN. You should not add a port that is already part of an Intel ANS VLAN to an LBFO team, as this may cause system instability.

# Configuring VLANs in Microsoft* Windows*

In Microsoft* Windows*, you must use Intel® PROSet to set up and configure VLANs. For more information, select Intel PROSet in the Table of Contents (left pane) of this window.

| Notes:

- A maximum of 64 VLANs per network port or team are supported by Intel PROSet.
- If you change a setting under the Advanced tab for one VLAN, it changes the settings for all VLANS using that port.
- ANS VLANs are not supported on adpaters and teams that have VMQ enabled. However, VLAN filtering with VMQ is supported via the Microsoft Hyper-V VLAN interface. For more information see Microsoft Hyper-V virtual NICs on teams and VLANs.
- You can have different VLAN tags on a child partition and its parent. Those settings are separate from one another, and can be different or the same. The only instance where the VLAN tag on the parent and child MUST be the same is if you want the parent and child partitions to be able to communicate with each other through that VLAN. For more information see Microsoft Hyper-V virtual NICs on teams and VLANs.