# DOS Troubleshooting

- Make sure you’re using the correct and most recent drivers for this adapter.

- If you’re replacing an existing adapter, make sure the LINK statement in your NET.CFG is correct for the new adapter.

- Verify that the frame type in your NET.CFG file matches your network.

- Test the adapter by running the DIAGS.EXE diagnostics program. Additional testing is
  available by using a responder.

`Last modified on 9/08/05 7:08a Revision 5`