This release note and the software that accompanies it are copyright (c) 2012, LSI Corporation or its suppliers, and may only be installed and used in accordance with the license that accompanies the software.

This Software is furnished under license and may only be used or copied in accordance with the terms of that license. No license, express or implied, by estoppel or otherwise, to any intellectual property rights is granted by this document. The Software is subject to change without notice, and should not be construed as a commitment by LSI CORPORATION or its suppliers to market, license, sell or support any product or technology. Unless otherwise provided for in the license under which this Software is provided, the Software is provided AS IS, with no warranties of any kind, express or implied. Except as expressly permitted by the Software license, neither Intel Corporation nor its suppliers assumes any responsibility or liability for any errors or inaccuracies that may appear herein. Except as expressly permitted by the Software license, no part of the Software may be reproduced, stored in a retrieval system, transmitted in any form, or distributed by any means without the express written consent of LSI CORPORATION.


===================
Package Information
===================
SNMP version = 14.11.01.00
Generic SNMP Agent version = 3.18.0.2
SAS-IR Data Collector version = 1.35.0.0
SAS-IR MIB File	version = 1.28-01
Storelibir version = 5.07.0.0
Storelibir-2 version = 20.0.0.0
Storelibir-3 version = 7.0.0.0
OS supported = Windows* 2000, Windows* 2003, Windows* XP, Windows* Vista, Windows* 2008, Windows* 7, Windows* 8 and Windows 2012
This package can be installed on all x86 and x64 systems.


=======================================
How to configure SNMP Agent in Windows:
=======================================
Step 1. Use SNMP Manager to retrieve the data (It is assumed that you have compiled mib files already). The mib files are available at the same location as setup.exe
 
Step 2. Use Trap utility to get the traps.

NOTE : Before you install the Agent, Make sure that SNMP Service is already installed in the system.

If you do not have SNMP Service installed on your system, Follow the following steps to install SNMP Service for Windows System.

Steps to install SNMP Service in Windows 2003:

Step 1. Select Add/Remove Programs from Control Panel.

Step 2. Select "Add/Remove Windows components" in the left side of the "Add/Remove Programs" window.

Step 3. Select "Management and Monitoring Tools".

Step 4. Click Next and SNMP service installation will start.

NOTE : In-between the installation you will be prompted to insert Windows 2003 CD, once you provide the CD and click OK the SNMP installation 
will resume and SNMP Service will be installed on that system. Once Installation is done, 
it will display a message saying Installation is successful

Steps to Configure SNMP Service on Server side

Step 1. Select "Administrative Tools" from Control Panel

Step 2. Select Services from "Administrative Tools" window.

Step 3. Select SNMP Service in the "Services" window.

Step 4. Open SNMP Service and go to its properties.

Step 5. Goto "Security" tab and make sure that "Accept SNMP Packets from any host" is selected. Add a community with some keyword. Eg-" public"

Step 6. Goto "Traps" tab and the list of host IPs to which you want the traps to be sent with community name.


=====================================================
Steps to install SNMP Service on Windows Server 2008:
=====================================================
Before you install the LSI Agent, Make sure that SNMP Service is already installed in the system.

If you do not have SNMP Service installed on your system, Follow the following steps to install SNMP Service for Windows 2008 System.

Step 1. Select Program and Features from Control Panel.

Step 2. Click on "Turn windows feature on/off" to select the windows components to install.

Step 3. Select Features in the left side menu.

Step 4. Click on Add Features.

Step 5. Select "SNMP Services".

Step 6. Click on Next.

Step 6. Click on Install and SNMP installation starts, You will be prompted for the Windows 2008 CD during the installation, 
Insert the CD and select OK, the installation will resume. Once Installation is done, 
it will display a message saying Installation is successful.

Follow the below Steps to Configure SNMP Service on Server side on Windows 2008.

Step 1. Select "Administrative Tools" from Control Panel

Step 2. Select Services from "Administrative Tools" window.

Step 3. Select SNMP Service in the "Services" window.

Step 4. Open SNMP Service and go to its properties.

Step 5. Goto "Security" tab and make sure that "Accept SNMP Packets from any host" is selected.Add a community with some keyword. Eg-" public".

Step 6. Goto "Traps" tab and the list of host IPs to which you want the traps to be sent with community name.

=====================================================
Steps to install SNMP Service on Windows Server 2012:
=====================================================
Before you install the LSI Agent, Make sure that SNMP Service is already installed in the system.

If you do not have SNMP Service installed on your system, Follow the following steps to install SNMP Service for Windows 2012 System.

Step 1. Select Program and Features from Control Panel.

Step 2. Click on "Turn windows feature on/off" to select the windows components to install.

Step 3. In server manager, select 'All servers'

Step 4. In installation type, select 'Role based or feature based installation'

Step 5. In server selection, select the server where SNMP services needs to be installed

Step 6. In features, select 'SNMP service' and click 'Add features'

Step 7. Click on 'Next' and 'Install' to finish installing SNMP service


Follow the below Steps to Configure SNMP Service on Server side on Windows Server 2012

Step 1. Select "Administrative Tools" from Control Panel

Step 2. Select Services from "Administrative Tools" window.

Step 3. Select SNMP Service in the "Services" window.

Step 4. Open SNMP Service and go to its properties.

Step 5. Goto "Security" tab and make sure that "Accept SNMP Packets from any host" is selected. Add a community with some keyword. Eg-" public".

Step 6. Goto "Traps" tab and the list of host IPs to which you want the traps to be sent with community name.


=============
Known Issues:
=============
For any set operation, user may need to wait 10-15 secs to see the changed value.

For a walk operation in Windows XP and Windows 2003 may shows "End of MIB" in HP-OV.

After Loading a MIB file in HPOV, close "Alarm Categories" window and then reopen it from Fault->Alarms.

If any previous installed HPOV present in which SAS mib loaded, then clean any existing LSI Trap definition from HPOV's trapd.conf [or, reinstall HPOV].


With the usage of the components version MR 5.8 or MR 6.1 firmware and MR5.5, 5.6, 5,7 & MR6.0 SNMP builds, 
the following issue is observed with 4k drives: Wrong value will be observed When user query for logical drive stripe size.
To avoid this issue use the latest MR 5.8 or MR 6.1 SNMP build.


==============
Fixes/Updates:
==============
14.11.00.01

MR 6.6

Defects:
1) SCGCQ00758121: SNMP ReadMe should be updated with OEL 7.0 support commands.

14.11.00.02

Enhancements:
1) SCGCQ00663903: End Customer: KDDIQuestion: According to the lsi-adaptersas.mib, 
		    KDDI think the severity of the below SNMP trap should be cr.  

14.11.00.03

Defects:

MR 6.6

1) SCGCQ00774873: MR6.6:SNMP: HOSTOSINFO showing N/A

SyncroCS 2.1

1) SCGCQ00762199: Syncro SSHA : MSM RHEL 6.5 -> Glibc detect /usr/sbin/lsi_mrdsnmpagent : malloc(): memory corruption error while install MSM. 

14.11.00.05

Repackaged with Latest SL, SLIR2 and SLIR3 Libraries.

14.11.01.00

Repackaged with Latest SL v4.30.1 and SLIR3 v7.00 Libraries.

Defects:

MR 5.13

1) SCGCQ00789202: Windows SNMP Compilation failed "MaintenanceMode" must start with lowercase letter" this is error in mib compiler